**November 25, 2019**

* Updated him on recent meeting with Frank and Machine Learning team
* Talked about keeping local database on the Pi to handle connection failure
  + Amir’s suggestion: Don’t keep local database; Handle connection failure by saving sensor data in file, for example